TITLE:

ANTIRUST ADVANCED - NEW FEATURES

POSITIONING OF THE NOZZLES ACCORDING TO THE TUBES/PROFILES DIMENSION

(Mettere immagine della macchina completa e della cassetta con i riferimenti di posizione)

INTRO - The new Antirust positioning feature (only available on Antirust Advanced) allows an easier regulation of the nozzles inside the spray box according to the size of the tubes/profiles to grant an even distribution of RPO on the product surface.

In this video we will see how to set the HMI and position the nozzles correctly.

00:00:00 – 00:00:07 Select “Auto” then touch the spray box on the HMI screen to access the configuration page

00:00:08 – 00:00:21 Select “New size” and input the credentials

(far uscire un pop up con le seguenti info:

User: operator

Password: 100

00:00:22 – 00:00:31 Touch “New size” again and input the size of the tubes/profiles of the new recipe in the top left corner of the HMI.

00:00:32 – 00:00:54 Select “Save” and put the name of the new recipe then select “Save” and “Send” (se possibile taglia l’errore di battitura di Tommaso dove scrive 84 passando direttamente a 83)

00:00:56 – 00:00:59 Saved recipe name

00:01:00 – 00:01:01 Suggested spray box size

00:01:02 – 00:01:06 Suggested nozzles location inside the spray box

00:01:07 – 00:01:18 Unlock the spray box and carefully unplug the connector (se possible inverti la sequenza facendo vedere prima lo sblocco e poi la rimozione del connettore (solo per dare un senso migliore alla frase, se non è possibile vedo come rigirare la frase)

00:01:19 – 00:01:32 Position the spray box on the dedicated trolley and secure it with the locking system.

00:01:33 – 00:01:52 Proceed with the regulation of the nozzles according to the indication on the HMI.

(Mettere un pop up con il ritaglio dello schermo che fa vedere il ditino che passa sulle varie posizioni)

A person's hand touching a computer screen

Description automatically generated

00:01:53 – 00:02:03 Tighten the nozzles in the selected position

00:02:04 – 00:02:17 Remove the adjusted spray box and place it back in the machine

00:02:18 – FINE Lock the spray box and carefully reconnect the plug

YOUR ANTIRUST IS FULLY SET AND READY TO GO!